;;	EditText.dat
;;
;;	2004/8/19

[SELECT_PARTS_DIALOG]
COUNT=1
TEXT1=Select your replaced or removed part(s), and detemine with OK button so that all of required adjustments will automatically be decided, and guide you in correct order.

[STATUS_MONITOR]
BitmapFile1=prnidle.bmp
BitmapFile2=prnerror.bmp

[INDIVIDUAL_LIST]
COUNT=1
TEXT1=Select an adjustment item from the below window. Then, double-click your target adjustment item to execute it.

[EEPROM_COPY]
COUNT=4
TEXT1=This function copies EEPROM data from current main board to new main board.
TEXT2=1) Click [Backup] button to backup EEPROM data from current main board.
TEXT3=2) Turn off the printer and replace current main board with new one.
TEXT4=3) Trun on the printer again and click [Restore] button.

[EEPROM_INITIALIZE]
COUNT=6
TEXT1=NOTE : Please perform this function only when EEPROM data is not backed up
TEXT2=       with EEPROM Data Copy function.
TEXT3=
TEXT4=1) Click [Initial setting] button to register initial setting value into EEPROM.
TEXT5=2) Input the Product Serial No. and click the [USB-ID input] button to register new USB-ID into EEPROM.
TEXT6=3) Click the [Check] button to read out current setting values.

[PF_DETERIORATION_OFFSET]
COUNT=1
TEXT1=1) Click [Initialization] button to reset current PF deterioration value to "Zero".

[PF_DETERIORATION_OFFSET_MAX]
COUNT=1
TEXT1=1) Click [Input] button to register the maximum PF deterioration value into EEPROM.

[HEAD_ID_INPUT]
BitmapFile1=headid.bmp
COUNT=7
TEXT1=[How to input Head ID]
TEXT2=1) Input Head ID on edit box.
TEXT3=2) Click [Input] button to register Head ID into EEPROM.
TEXT4=     If error message is displayed, please input Head ID again.
TEXT5=
TEXT6=[How to check current Head ID]
TEXT7=1) Click [Check] button to check current Head ID.

[HEAD_ANGULAR]
COUNT=7
TEXT1=1) A4/Letter size of Plain Paper on ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=       - Band pattern
TEXT4=       - Raster Offset pattern
TEXT5=3) Select the best pattern from each check pattern.
TEXT6=4) Select the parameter of the selected pattern on edit box.
TEXT7=5) Click [Input] button to register the parameter into EEPROM.

[MANUAL_BID]
COUNT=9
TEXT1=1) A4/Letter size of Plain Paper on ASF.
TEXT2=2) Click [Print] button to print check pattern of selected PG & selected dot size.
TEXT3=3) Select the best pattern from each check pattern.
TEXT4=4) Select the parameter of the selected pattern on edit box.
TEXT5=5) Click [Input] button to register the parameter into EEPROM.
TEXT6=     In case that there is no best pattern, you have to input the maximun or 
TEXT7=     mininum parameter in the check pattern once. Due to this, the check pattern
TEXT8=     with offset value is printed in the center position of next check pattern print.
TEXT9=     Please repeat this adjustment until you can select the best pattern.

[FIRST_DOT]
COUNT=9
TEXT1=1) A4/Letter size of Economy Photo Paper/Glossy Photo Paper on ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=3) Select the best line with the following procedure from each check pattern.
TEXT4=4) Select the parameter of the selected pattern on edit box.
TEXT5=5) Click [Input] button to register the parameter into EEPROM.
TEXT6=
TEXT7=[How to select the best line]
TEXT8=1) Select the printed line on 5mm away from each edge of paper.
TEXT9=2) Select the parameter of the selected pattern on edit box.

[PW_ADJUSTMENT]
COUNT=9
TEXT1=1) A4 size of Economy Photo Paper/Glossy Photo Paper on ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=3) Select the best line with the following procedure from each check pattern.
TEXT4=4) Select the parameter of the selected pattern on edit box.
TEXT5=5) Click [Input] button to register the parameter into EEPROM.
TEXT6=
TEXT7=[How to select the best line]
TEXT8=1) Select the printed line on 5mm away from each edge of paper.
TEXT9=2) Select the parameter of the selected pattern on edit box.

[PF_ADJUSTMENT]
COUNT=7
TEXT1=1) A4 size of Economy Photo Paper/Glossy Photo Paper on ASF.
TEXT2=2) Click [Print] button to print check pattern.
TEXT3=3) Select the best pattern from the check pattern.
TEXT4=4) Select the parameter of the selected pattern on edit box.
TEXT5=5) Click [Input] button to register the parameter into EEPROM.

[HEAT_PROTECTION]
BitmapFile1=Caution.bmp
COUNT=6
TEXT1=1) Select replacement parts from the following check boxes.
TEXT2=    Please do not perform this adjustment without replacing the affected parts
TEXT3=    with new one.
TEXT4=2) Click [Perform] button to register the proper value of CR motor heat protection 
TEXT5=    into EEPROM according to the selected replacement parts. (For this operation,
TEXT6=    it takes about 1 min.)

[CLEANING]
COUNT=4
TEXT1=1) Click [Print] button to print nozzle check pattern print.
TEXT2=2) If dot missing appers, click [Cleaning] button to perform the cleaning.
TEXT3=3) Click [Print] button to print nozzle check pattern print again.
TEXT4=4) If dot mssing is not recovered, repeat from step 2) to step 3) 

[INK_CHARGE]
COUNT=5
TEXT1=1) Click [Ink Charge] button to perform ink charge.
TEXT2=2) Click [Print] button to print nozzle check pattern print.
TEXT3=3) If dot missing appers, click [Cleaning] button to perform the cleaning.
TEXT4=4) Click [Print] button to print nozzle check pattern print again.
TEXT5=5) If dot mssing is not recovered, repeat from step 3) to step 4) 

[INK_PAD_COUNTER]
COUNT=6
TEXT1=NOTE : You have to replace waste ink pad with new one once you initialize
TEXT2=             the protection counter.
TEXT3=
TEXT4=1) Click [Check] button to check current protection counter.
TEXT5=2) Replace waste ink pad with new one.
TEXT6=3) Click [Initialization] to reset current protection counter to "Zero".

[SHIPPING_SETTING]
COUNT=5
TEXT1=This function will have a cleaning process performed automatically when the printer is turned on.
TEXT2=1) Please implement this function in case of nozzle expulsion troubles caused by the transport. When clicking the "Write" button, the shipping settings are entered in the machine.
TEXT3=2) The shipping settings will be registered when the printer is turned off and applied directly the next time it is turned on.
TEXT4=Attention:
TEXT5=The function resets the shipping settings if the printer is turned on. In this situation, it is necessary to implement the shipping settings once again before turning off the power.

[CHECK_PATTERN_PRINT]
COUNT=1
TEXT1=1) Click [Print] button to print selected pattern.

[CDR_CHKPAT_PRINT]
COUNT=1
TEXT1=1) Click [Print] button to print CD-R check pattern.

[EEPROM_READOUT]
COUNT=1
TEXT1=1) Click [Dump] button to read out and save all of EEPROM data.

[OPERATION_INFO]
COUNT=1
TEXT1=1) Click the [Check] button to read out the printer information.
